assemble with ASM.COM or MAC.COM

ASM CPM22

This generates CPM22.HEX with a few extra addresses in the F600 (BIOS)space.
Either delete these or upload the BIOS _after_ CPM22. BIOS will overwrite these.
