Romimage\_Feb28\_2009\_TOOLS\_Zork.bin as uploaded by nbreeden

B:\  
 format.com rtc.com xmodem.com

F:\  
 2400.mac 38400.mac asm.com bascom.com baslib.rel bcload  
 brun.com ddt.com ddtz.com dirx.com dump.com ed.com  
 formata.com formatb.com keyboard.com l80.com lcd20x4.com  
 lib80.com load.com lu.com m80.com mbasic.com pip.com  
 pmautoae.com r.com simple.com speed.com stat.com  
 supersub.com survey.com unload.com vde263.com vedit.com  
 vinst263.com w.com ws.com ws.ovr wsmsgs.ovr  
 wsprint.ovr wsu.com xiz.com xm.com xm50lb1.com   
 xmodem38.com xsub.com xzi.com zde.com zork1.com  
 zork1.dat zork2.com zork2.dat zork3.com zork3.dat

Instructions for Romimage\_Feb28\_2009\_TOOLS.bin

1. Target is a 27C801 (8MB) EPROM
2. This is the image Romimage\_Feb28\_2009.bin with additional files added to drive F:
3. 38400 baud bootup, Drive A-Ram, B=ROM, warm boot skips cpm reload, added tsr routines, show warm boot message, add autoexec and supersub
4. Not enabled – no ide delay (ie set up to use IDE drives if needed), keyboard not enabled, echo off not enabled (only used for radio)